// Het programmablok void setup wordt eenmaal beschreven
void setup () {
   pinMode(2, OUTPUT);     // We geven aan dat de led-pin-aansluiting een output is (spanning moet geven)
   pinMode(3, OUTPUT);     // We doen hetzelfde voor alle led-pin-aansluitingen
   pinMode(4, OUTPUT);
   pinMode(5, OUTPUT);
   pinMode(6, OUTPUT);
   pinMode(7, OUTPUT);
   pinMode(8, OUTPUT);
   pinMode(9, OUTPUT);
 }

// Het programmablok void loop herhaalt zich keer op keer
void loop () {
   digitalWrite(2,HIGH);   //signaal hoog op led-pin-aansluiting 2 (led is aan)
   delay(100);		   //wachten 100 ms
   digitalWrite(3,HIGH);   
   delay(100);
   digitalWrite(4,HIGH);
   delay(100);
   digitalWrite(5,HIGH);
   delay(100);
   digitalWrite(6,HIGH);
   delay(100);
   digitalWrite(7,HIGH);
   delay(100);
   digitalWrite(8,HIGH);
   delay(100);
   digitalWrite(9,HIGH);
   delay(100);
   digitalWrite(9,LOW);
   delay(100);
   digitalWrite(8,LOW);
   delay(100);
   digitalWrite(7,LOW);
   delay(100);
   digitalWrite(6,LOW);
   delay(100);
   digitalWrite(5,LOW);
   delay(100);
   digitalWrite(4,LOW);
   delay(100);
   digitalWrite(3,LOW);
   delay(100);
   digitalWrite(2,LOW);
   delay(100);
}
