## Testing the weather station

In order for the weather station to authenticate itself to the TTN, the generated AppKey must be entered in the main.py program of the Raspberry Pi Pico (H).

Once this has been done, you can test whether data is being transmitted from the weather station to the TTN .In order for the weather station to authenticate itself to the TTN, the generated AppKey must be entered in the main.py program of the Raspberry Pi Pico (H).

Once this has been done, you can test whether data is being transmitted from the weather station to the TTN .

firmware vetskilling.zip

If the weather station has sent sensor data to the TTN, you can log in to TTN and see in the application window whether the data has been received.

The Forward uplink data message lines show the data received.

If the weather station has sent sensor data to the TTN, you can log in to TTN and see in the application window whether the data has been received.

The Forward uplink data message lines show the data received.